Seal Shaft Section:

* Lox side Bearing ID = .472 in, interference = 0-2 um = .00007in holy shit we are not hitting that.
* Lox side height = .786 inches. Skf recoments .787 in for centerline of coolant nozzle, clearance = .002in
* Kerosene side